AsTher - Process Calculator for MS Excel

AsTher Thermodynamic Database and Applications

| home |

AsTher Process Calculator for MS Excel

5.3. Carbon gasification by Water. Create graphics for different variable
Download file C-H2O.xls

5.3.1. Condition Sheet

The green coloured cells are written by user before calculation.

Cell [B3]=300+B6*50 means, that after each calculation temperature will be increased in depend of calculation count.
Cell [B3]=1 calculations are carried out for 1 bar.
Cell [B4],[C4] sheet names for the phase is written.

Cell [B6] 0: reset calculations.
Cell [C6] calculations are carried out 20 times.

Cell [B10] * : means if the calculation count is less than 20, then the next calculations system is defined in the same file.
Cell [C10] * : means if the calculation count is less than 20, then the next calculations system is defined in the same condition sheet.

Cell [B12] P_1bar:Calculations result is written in the sheet named P_1bar, the sheet must exist in the same file (or in the same MS Excel book)

Cells [B13] to [B25]: the cells contain links to another cell in different sheet, which data are recorded in the sheet P_1bar

5.3.2. Sheet for Phase gas

The green coloured cells are written by user before calculations.

Cell [B9] contains input value for H2O (g) 1 [mol].

5.3.3. Sheet for Phase solid

The green coloured cells are written by user before calculations.

Cell [B1] contains input value for C (s) 1 [mol].

5.3.3. Calculations

Execute AsTher Process Calculator for MS Excel (XProCalc.exe).
Select as MS Excel file C-H2O.xls
Select as condition sheet Cond
Press button Calculation

5.3.3. Recorded data

5.3.3.1. Calculation results in depend of the temperature

The sheet named P_1bar, contains no any data before calculations.
While calculations, the following data is written by AsTher Process Calculator for MS Excel (XProCalc.exe)in the sheet P_1bar.

Graphic Charts can created by user.

5.3.3.2. Calculation results in depend of the pressure

In the sheet Cond, the following data are written, before calculations.

Cell [B3]=600 calculations are carried out for 600[C].
Cell [B3]=0.1+B6*0.1 means, that after each calculation pressure will be increased in depend of calculation count.

Cell [B6] 0: reset calculations.
Cell [C6] calculations are carried out 20 times.

Cell [B13] T_1000C:Calculations result is written in the sheet named T_600C, the sheet must exist in the same file (or in the same MS Excel book)

Cells [B14] to [B25]: the cells contain links to another cell in different sheet, which data are recorded in the sheet T_600C

The sheet named T_600C, contains no any data before calculations.
While calculations, the following data is written by AsTher Process Calculator for MS Excel (XProCalc.exe) in the sheet T_600C.